Help
To store changed settings click on "Apply" at the bottom of the page.
The device will restart with the new setting.
Max. output volume
The max. audio output level is configured here. Volume control via any of the interfaces will cover the range of 0... this configured parameter. Choose between "0"% and "100"% in 5% steps.
Default: "50"%
Input gain
On hardware with audio input, this controls the input gain of the analog input.
Default: "0dB"
Input attenuation with message
On hardware with audio input, controls how much the input signal will be attenuated when a message is played.
Default: "0%"
UDP Command Port
Selects the UDP port number on which the device will wait for commands (0 to disable the UDP interface).
Default: "0"
Resistor Value
The value (in Ohm) of resistor that you use for chain connected to "signal ground" of X8 (Pin 1 of J1). All resistors (up to 9) in this chain must have the same this value. Player will automatically calculate the proper voltages in this chain on the base of this value and define the proper closed button (from 0 up to 9) for inputs I1-I7 (Pins 8-2 of J1). To avoid the possible mistakes with button recognition it is recommended to use the value from 500 to 3000 Ohm (optimal 1000 Ohm).
Default: "1000"