HOME "); &LSetup(3,"%s",180,S,"sip_rava","-->"); &LSetup(3,"%s",180,S,"ip_intercom","-->"); | PROFILES &LSetup(3,"%s",180,S,"ip_intercom"," "); | CUSTOM1 TAB &LSetup(3,"%s",180,S,"custom1"," | CONFIGURATION "); | CONTROL &LSetup(3,"%s",180,S,"tunnel_msgr"," | STATUS | DEFAULTS | UPDATE | REBOOT | &LState(1,"%u",28); MAC: &LState(1,"%s",12); FW V&LSetup(5,"%02x");.&LSetup(6,"%02x");
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
&LSetup(3,"%s",180,S,"ip_intercom","IP INTERCOM"); &LSetup(3,"%s",180,S,"sip","SIP CLIENT"); &LSetup(3,"%s",180,S,"sip_rava","SIP-RAVA&trade\; CLIENT &LBAS(1,\"%fs\",ver$)\;"); &LSetup(3,"%s",180,S,"sip_tvc","Televic SIP IP Gateway &LBAS(1,\"%fs\",ver$)\;"); &LSetup(3,"%s",180,S,"sip_paviro","Bosch Paviro SIP IP Gateway &LBAS(1,\"%fs\",ver$)\;"); &LSetup(3,"%s",180,S,"tinker","JDACCS RID Configuration UI"); &LSetup(3,"%s",180,S,"tunnel_msgr","TUNNEL MESSENGER"); &LSetup(3,"%s",180,S,"dcr_fire","DCR FIRE STATION"); &LSetup(3,"%s",180,S,"custom1","CUSTOM1 APPLICATION"); &LSetup(3,"%s",180,S,"asx","ASX Intercom System"); &LSetup(3,"%s",180,S,"any2all","Any to All PA System"); &LSetup(3,"%s",180,S,"icmaster","Intercom Master Station"); &LSetup(3,"%s",180,S,"icclient","Intercom Client Station"); &LSetup(3,"%s",180,S,"bgm_client","Background Music Client"); &LSetup(3,"%s",180,S,"pagingzone","Paging Zone"); &LSetup(3,"%s",180,S,"annunfdx","Full-duplex Intercom"); &LSetup(3,"%s",180,S,"lradx","LRAD - PA and Alerting System"); &LSetup(3,"%s",180,S,"simplepg","Simple Paging"); &LSetup(3,"%s",180,S,"pae-ip","PAE-IP &LBAS(1,\"%fs\",ver$)\; - Device: &LSetup(4,\"%s\",98)\; (IP: &LState(1,\"%s\",13)\;)"); |