'0202
'----------------------------------------------------------------------------------------------
' 
' any2all project
'
' Angelo Dureghello
'   Barix AG, 
'     08.07.2009, Trieste, Italy
'
'
'  00.01  20.08.09 AD  ant2all Initial Version.
'  00.02  31.08.09 AD  ! fixed  local listening port.
'  00.03  05.02.10 DB  + added support for Annuncicom 200 (HW:19).
'  01.00  09.02.12 AD  c chged new ABCL web UI style.
'                      + added colored input state display, white,lime,gray, with 
'                        white/unavailable detection.
'                      + added configurable multicast listening address.
'                      + added G711 audio formats, 8 and 24Khz.
'                      c chged rx buffer in bytes to RTP delay.
'                      + added ASCII discovery, as udp reply to port 12301, command: c=65535.
'  02.00  29.02.12 AD  c chged abcl backend layer to support IPAM102.
'                      + added (#075.07) RTP payload detection, in/out stream status.
'                      + added (#075.08) RTP statistics and stream from.
'                      + added (#075.10) application status details added inside status page.
'                      + added (#075.06) destination table to a total of 16 destinations,
'                              X8 connection always allowed in every device.
'                      + added (#075.06) PS16 support.
'  02.02  02.10.18 ASI ! fixed (#ANY2ALL-18) extended the broadcast to 14 streams
'                      + added (#ANY2ALL-17) activation of LED for pressed buttons
'         12.11.18 ASI ! fixed Updated the date of the application to correspond to the 
'                              release date
'----------------------------------------------------------------------------------------------
'
dim ver$(24)

