&LSetup(3,"%s",130,D,0," ");

NETWORK SETTINGS
Use SonicIP® | Yes No
IP Address | . . .
Netmask | . . .
Gateway IP Address | . . .
Primary DNS | . . .
Alternative DNS | . . .
Syslog Address | . . .
DHCP Host Name |
Web Server Port | ");&LState(2,"%s",28,17,"-->");
Default Ethernet Port |

STREAMING SETTINGS
Target table
# | Input | IP Address | Port
1 | Device I0 | . . . : |
2 | Device I1 | . . . : |
3 | Device I2 | . . . : |
4 | Device I3 | . . . : |
5 | Device I4 | . . . : |
6 | Device I5 | . . . : |
7 | Device I6 | . . . : |
8 | Device I7 | . . . : |
9 | X8 I0 / PS16 I8 | . . . : |
10 | X8 I1 / PS16 I9 | . . . : |
11 | X8 I2 / PS16 I10 | . . . : |
12 | X8 I3 / PS16 I11 | . . . : |
13 | X8 I4 / PS16 I12 | . . . : |
14 | X8 I5 / PS16 I13 | . . . : |
15 | X8 I6 / PS16 I14 | . . . : |
16 | X8 I7 / PS16 I15 | . . . : |
INCOMING STREAM
Receiving Socket | . . . : |
RTP delay |

AUDIO SETTINGS
Output Volume | %
Input Source | Line Mic
Microphone Gain | dB
A/D Amplifier Gain | dB
Audio Format |
MPEG Encoding Quality |
Sample Rate |

I/O
X8 Connection Port | COM 1 COM 2
Relay Action |

SECURITY SETTINGS
Reset Function | Enabled Disabled
Factory Defaults | Enabled Disabled
Update Function | Enabled Disabled
&LSetup(3,"%s",130,D,0," Set Password | "); &LSetup(3,"%s",130,D,!0," | Old Password |
New Password | ");