Home Page Application Status This section shows the actual application state. The displayed field list is reported below. Note: see the system status page for further details on the actual device configuration. State Displays the current application state. X8 Extension Displays if the Barix X8 extension is connected or not. Device Inputs Displays the current device digital input states. X8 Inputs Displays the current Barix X8 digital input states. Relay State Display current relay state. Note: I/O states are updated once per second and displayed with colored boxes, with the following meaning: lime : active, contact closed gray : inactive, contact open white : unavailable Note: when the application run on Barix PS16 Paging Station, device input states from 1 to 8 corresponds respectively to the states of PS16 1 to 8 keys, while X8 input states, from 1 to 8, corresponds respectively to the states of PS16 9 to 16 keys. Decoding Audio Format Displays current decoding audio format, detected from the incoming stream RTP payload type. Encoding Audio Format Displays current encoding audio format. Average Bitrate If the device is receiving, displays average bitrate, as kbits per second. RX Buffer Level If the device is playing, displays the current audio buffer level, in bytes, from 0 to a maximum of 32768. Current Volume Current volume level, from 0 to 100%, as 5% steps. Input Level Displays current audio input level, as linear value, from 0 to a maximum of 32768. Output Level Displays current audio output level, as linear value, from 0 to a maximum of 32768. RTP Lost Frames Number of lost frames during decoding. The value is reset with every new RTP sequence. RTP Duplicated Frames Number of duplicated frames during decoding due to the buffer management. Frames are duplicated if encoder is slower than decoder. RTP Dropped Frames Number of dropped frames during decoding due to the buffer management. Frames are dropped if encoder is faster than decoder.