Application Status
Current State : |
X8 State : | &LBAS(1,"%fs",x8st$);
I/O States
Device Inputs (0 to 7): |
X8 Inputs (0 to 7): |
Relay State : | &LBAS(1,"%lu",relst);
Streaming Details
Decoding Audio Format : |
Encoding Audio Format : |
Average Bitrate : | &LBAS(1,"%lu",fps); Kbit/sec
RX Buffer Level : | &LBAS(1,"%lu",bufl); Bytes
Current Volume : | &LSetup(1,"%u",500); (5% steps)
Input Level : | &LBAS(1,"%lu",inl);
Output Level : | &LBAS(1,"%lu",outl);
RTP Lost Frames : | &LBAS(1,"%lu",flst);
RTP Duplicated Frames : | &LBAS(1,"%lu",fdup);
RTP Dropped Frames : | &LBAS(1,"%lu",fdro);