Help Basic Settings Basic settings, for a fast configuration of the PA system. Streaming sockets (IP and ports) can be configured here. Target Table This table allows to use digital inputs to start and stop streaming to a destination. For every available input is possible to configure a destination socket (IP:PORT). IP as 0.0.0.0, or a port value set to 0, mean "no target". Unicast, or multicast IP addresses can be used here. By having a destination address of 255.255.255.255 configured against an input, the device will stream to ALL destinations configured in the target table when that input is activated. The streams will be sent UNICAST to each destination. Note: on Barix PS16 Paging Station the 16 destinations corresponds, from n. 1 to 16, to PS16 keys 1 to 16. [default: 0.0.0.0 : 0] Receiving Socket Audio stream receiving socket (IP:PORT). Use 0.0.0.0 (default) to listen to any IP or use a multicast IP to join a multicast group. [default: 0.0.0.0 : 3030]