&LSetup(3,"%s",130,D,0," ");

NETWORK SETTINGS
Use SonicIP® | Yes No
IP Address | . . .
Netmask | . . .
Gateway IP Address | . . .
Primary DNS | . . .
Alternative DNS | . . .
Syslog Address | . . .
DHCP Host Name |
Web Server Port | ");&LState(2,"%s",28,17,"-->");
Default Ethernet Port |
SNMP System Name |
SNMP System Location |
SNMP System Contact |

BARP CONTROL
BARP Station ID |
BARP Broadcast Address | . . .
BARP Audio Port |
BARP Control Port |
BARP Status Port |
Notification Port | No Yes
Notification Broadcast Port |
Notification Protocol |

AUDIO
Audio Format |
Acoustic Echo Cancellation | On Off
Input Source | Line Mic
Duplex Mode | Half Full
Use AI_Phone | No Yes
Microphone Gain | dB
A/D Amplifier Gain | dB
Default Paging Volume | %
Minimal Paging Volume | %
Maximal Paging Volume | %
Default BGM Volume | %
Minimal BGM Volume | %
Maximal BGM Volume | %
Notification Volume | %

OUTGOING CALL
Call Master by | IP Address BARP ID
Master Station 1 IP | . . .
Master Station 2 IP | . . .
Master Station 3 IP | . . .
Master Station 4 IP | . . .
Master Station 1 ID |
Master Station 2 ID |
Master Station 3 ID |
Master Station 4 ID |
Call next Master | No Yes
Auto Hang Up | secs

BACKGROUND MUSIC
BGM Broadcast Address | . . .
BGM First Broadcast Port |
BGM Available Channels |
BGM Start Channel |

SERIAL
Serial Port |
VSC Font Size |
VSC Panel Dim Timeout |

I/O CONTROL
Relay 1 Control |
Relay 1 Off Delay | milliseconds
LED Status |

SECURITY SETTINGS
Reset Function | Enabled Disabled
Factory Defaults | Enabled Disabled
Update Function | Enabled Disabled
&LSetup(3,"%s",130,D,0," Set Password | "); &LSetup(3,"%s",130,D,!0," | Old Password |
New Password | ");