'
' IcClient
'
' V01.00  05.06.12 AD    new started up from iclient 00.42.
'                        + added base ABCL fw upgrade to work with IPAM102.
'                        + added in/out levels.
'                        c chged web UI to new web UI look and feel.
' V01.01  25.06.12 AD    ! fixed web ui syntax errors.
'                        ! fixed iclient call next master not working when using ID's.
'                        c chged msg 3 (PA) timeout to  10000 (> 2x4secs intervals).
'                        ! fixed hdx unattended receiving from state 4(intercom).
' V01.02  04.07.12 AD    ! fixed web UI home page help syntax.
'                        ! fixed delayed audio in FD after call established.
' V01.03  10.07.12 AD    ! fixed high latency on master side in IC mode.
'                        ! fixed regression IC call not working properly after BGM.
'                        c chged to greater file chunks to be read for ring tone.
' V01.04  28.08.12 AD    ! fixed various web ui syntax errors.
'                        ! fixed bug #110.06 glitches on audio issue.
'                        ! fixed audio format not available for decoder only.
'                        + added mechanism to exit for timeout on established call.
' V01.05  10.09.12 AD    + added echo cancellation feature (AEC).
' V01.06  25.10.12 AD    c chged #110.09 paging/ic method using link.
'                        c chged #110.12 paging volume to be separated from bgm volume.
'                        + added routines with link timeout mechanism.
'                        ! fixed #109.01 mechanism to exit HD TX if master crash.
'                        ! fixed non working channel 0 local line input.
' V01.07  31.01.13 AD    + added new debug trace preprocessor macroes.
'                        + added tuned rtp delay on vlsi1053 to avoid stream timeout in pa.
'                        c chged no link for paging.
'                        ! fixed ICG not able to start spontaneous intercom.
'                        ! fixed client timeout to idle when in HD TX (ICG is in intercom RX).
'                        ! fixed #110.16, added BARP flags for extended timout checks.
'                        ! fixed #110,17, application receive and play multiple streams.
'                        ! fixed BGM audible when switching back to low priority page,
'                                reported from SG report 1.09 point 4.5.
'                        ! fixed BGM not starting on local channel at first boot,
'                                reported from SG report 1.09 point 6.2.
'                        ! fixed relay not closed while receiving paging,
'                                reported from SG report 1.09 point 8.4.
'                        ! fixed #110.02 false call starts on Annuncicom 200.
'                        + added payload/codec/delay detection for notification messages.
'                        + added BGM state on web UI.
'                        + added NOTIFICATION state on web UI.
' V01.08  13.11.13  AD   ! fixed cellpadding to 5 in icclient_uihadvanced.html.
'                        ! fixed Annuncicom 60 to be enc + dec.
' V01.09  19.08.14  ASI  + Added VSC font size setting on the webUI
' V01.10  20.08.14  ASI  + Added VSC panel dim on configurable timeout
'         21.08.14  ASI  + Adapt to use VSC dim timeout set by drop down menu on the webUI
' V01.11  23.10.14  ASI  + feature request #110.34: Add BGM stream detection and feedback 
'                          to the webUI
'	  24.10.14  ASI  ! fixed #110.35: No min/max volume check
' V01.12  10.11.14  ASI  ! fixed to show correctly "IDLE" on the webUI when no BGM is
'                          configured
' V01.13  15.01.15  ASI  ! fixed bug #110.31: The client relay 1 does not switch off after
'                          call end when set to "on while receiving stream"
' 

