Help BARP Station ID Enter here the BARP system ID of this master station. The ID is used from the clients to identify the source of the control messages in multimaster environment. Default setting is "1001". Duplex Mode Choose the desired mode of operation. Default setting is "Full". Hands Free When set to yes, and HDX mode is enabled, the talk/listen mode can be voice controlled. In Intercom mode, if the voice level exceeds the one set in "Input Trigger Level", the master is switching in talk mode, and the client in listen mode. In Page mode, the Page key needs to be pressed once (instead of press and hold) to activate the paging, and pressed again to stop. Default setting is "No". Hands Free Keys The function of the keys changes depending upon the device and the configuration (Full/Half duplex):
Function | FD Key | HD Key
PS16
Accept Call (IC) | 1 | 1
Reject Call (IC) | 3 | 3
Close Call (IC) | 1 or 3 | 3
Open Relay (IC) | 2 | 2
Start Paging | 2 (blinks whilst Paging)
Stop Paging | 2
PS1 and other 2 button Annuncicoms
Accept Call (IC) | A(1) | A(1)
Close Call (IC) | A(1) | A(1)+B(2)
Open Relay (IC) | B(2) | B(2)
Start Paging | B(2)
Stop Paging | B(2)
Group 1 Address Map Configures the address bitmask containing the clients to be paged for that group. Up to 128 clients may be selected, and the current number of the selected clients for each group is shown. Click on the corresponding "View/Modify" button to open the map configuration page for this group. Default is all "1 to 10" selected.