NETWORK
Use SonicIP: &LSetup(3,"%s",198,b7,0,"Yes");&LSetup(3,"%s",198,b7,1,"No");
IP Address: &LSetup(1,"%u",0);.&LSetup(1,"%u",1);.&LSetup(1,"%u",2);.&LSetup(1,"%u",3);
Netmask: &LSetup(2,"%u",8,0);.&LSetup(2,"%u",8,1);.&LSetup(2,"%u",8,2);.&LSetup(2,"%u",8,3);
Gateway IP Address: &LSetup(1,"%u",4);.&LSetup(1,"%u",5);.&LSetup(1,"%u",6);.&LSetup(1,"%u",7);
Primary DNS: &LSetup(1,"%u",64);.&LSetup(1,"%u",65);.&LSetup(1,"%u",66);.&LSetup(1,"%u",67);
Alternative DNS: &LSetup(1,"%u",68);.&LSetup(1,"%u",69);.&LSetup(1,"%u",70);.&LSetup(1,"%u",71);
Syslog Address: &LSetup(1,"%u",200);.&LSetup(1,"%u",201);.&LSetup(1,"%u",202);.&LSetup(1,"%u",203);
DHCP Host Name: &LSetup(4,"%s",98);
Web Server Port: &LSetup(1,"%u",283,W);
Default Ethernet Port: &LSetup(1,"%u",96);
SNMP System Name: &LSetup(4,"%s",205);
SNMP System Location: &LSetup(4,"%s",223);
SNMP System Contact: &LSetup(4,"%s",242);
BARP CONTROL
BARP Station ID: &LSetup(1,"%u",540,W);
BARP Broadcast Address: &LSetup(1,"%u",878);.&LSetup(1,"%u",879);.&LSetup(1,"%u",880);.&LSetup(1,"%u",881);
BARP Audio Port: &LSetup(1,"%u",852,W);
BARP Control Port: &LSetup(1,"%u",854,W);
BARP Status Port: &LSetup(1,"%u",856,W);
Notification Port: &LSetup(1,"%u",849,W);
Notification Broadcast Port: &LSetup(1,"%u",850,W);
Notification Protocol: &LSetup(3,"%s",529,b1,1,"RTP");&LSetup(3,"%s",529,b1,0,"Raw UDP");
AUDIO
Audio Format: &LSetup(3,"%s",511,B,6,"µ-law 24kHz");&LSetup(3,"%s",511,B,7,"µ-law 8kHz");&LSetup(3,"%s",511,B,8,"A-law 24kHz");&LSetup(3,"%s",511,B,9,"A-law 8kHz");
Acoustic Echo Cancellation: &LSetup(3,"%s",826,B,1,"On");&LSetup(3,"%s",826,B,0,"Off");
Input Source: &LSetup(1,"%u",510,B); (129=line, 130=mic)
Duplex Mode: &LSetup(1,"%u",830,B); (0=Full)
Use AI_Phone: &LSetup(1,"%u",831,B);
Microphone Gain: &LSetup(1,"%u",502,B); dB
A/D Amplifier Gain: &LSetup(1,"%u",501,B); dB
Default Paging Volume: &LSetup(1,"%u",500,B); 5% steps
Minimal Paging Volume: &LSetup(1,"%u",503,B); 5% steps
Maximal Paging Volume: &LSetup(1,"%u",504,B); 5% steps
Default BGM Volume: &LSetup(1,"%u",517,B); 5% steps
Minimal BGM Volume: &LSetup(1,"%u",518,B); 5% steps
Maximal BGM Volume: &LSetup(1,"%u",519,B); 5% steps
Notification Volume: &LSetup(1,"%u",840,B); 5% steps
OUTGOING CALL
Call Master by: &LSetup(3,"%s",874,B,0,"IP Address");&LSetup(3,"%s",874,B,1,"BARP ID");
Master Station 1 IP: &LSetup(1,"%u",530);.&LSetup(1,"%u",531);.&LSetup(1,"%u",532);.&LSetup(1,"%u",533);
Master Station 2 IP: &LSetup(1,"%u",540);.&LSetup(1,"%u",541);.&LSetup(1,"%u",542);.&LSetup(1,"%u",543);
Master Station 3 IP: &LSetup(1,"%u",858);.&LSetup(1,"%u",859);.&LSetup(1,"%u",860);.&LSetup(1,"%u",861);
Master Station 4 IP: &LSetup(1,"%u",862);.&LSetup(1,"%u",863);.&LSetup(1,"%u",864);.&LSetup(1,"%u",865);
Master Station 1 ID: &LSetup(1,"%u",866,W);
Master Station 2 ID: &LSetup(1,"%u",868,W);
Master Station 3 ID: &LSetup(1,"%u",870,W);
Master Station 4 ID: &LSetup(1,"%u",872,W);
Call next Master: &LSetup(1,"%u",875,W);
Auto Hang Up: &LSetup(1,"%u",544,B); secs
BACKGROUND MUSIC
BGM Broadcast Address: &LSetup(1,"%u",832);.&LSetup(1,"%u",833);.&LSetup(1,"%u",834);.&LSetup(1,"%u",835);
BGM First Broadcast Port: &LSetup(1,"%u",836,W);
BGM Available Channels: &LSetup(1,"%u",838,B);
BGM Start Channel: &LSetup(1,"%u",839,B);
SERIAL
Serial Port: &LSetup(3,"%s",199,B,0,"BCL Application");&LSetup(3,"%s",199,B,1,"VSC Panel");&LSetup(3,"%s",199,B,2,"RTC Module");
I/O CONTROL
Relay 1 Control: &LSetup(3,"%s",848,B,0,"always off"); &LSetup(3,"%s",848,B,2,"on while talking (in a call)"); &LSetup(3,"%s",848,B,3,"always on,off while in a call"); &LSetup(3,"%s",848,B,4,"on while in PA mode"); &LSetup(3,"%s",848,B,5,"on while receiving audio stream");
Relay 1 Off Delay: &LSetup(1,"%u",545,W); milliseconds
SECURITY SETTINGS
Reset Function: &LSetup(3,"%s",97,b0,0,"Enabled");&LSetup(3,"%s",97,b0,1,"Disabled");
Factory Defaults: &LSetup(3,"%s",97,b1,0,"Enabled");&LSetup(3,"%s",97,b1,1,"Disabled");
Update Function: &LSetup(3,"%s",97,b2,0,"Enabled");&LSetup(3,"%s",97,b2,1,"Disabled");
Password: &LSetup(3,"%s",130,D,0,"Is not set);&LSetup(3,"%s",130,D,!0,"Is set");