Help NETWORK SETTINGS Use SonicIP If set to "yes", the device will announce its IP address over the audio output during device startup. Default: "yes" IP Address Enter the 4 values of the desired device IP address e.g.: "0.0.0.0" for automatic discovery (DHCP/BOOTP, IPzator, AutoIP) "192.168.0.12" for an internal LAN Default: "0.0.0.0" Netmask Enter the 4 values of the desired Static IP e.g.: "0.0.0.0" for a default Netmask depending on the used IP Address. "255.255.255.0" for a C class network Default: "255.255.255.0" Gateway IP Address Enter the 4 values of the desired Gateway IP address e.g.: "0.0.0.0" for no Gateway "192.168.0.1" for a Gateway in a LAN Note: The Gateway has to be set only when connecting to other devices over the WAN (through a router). Default: "0.0.0.0" Primary DNS In this field you can give the device the desired primary and alternative DNS IP address to be able to connect to URLs (e.g. www.radio.com). Example: "195.186.1.111" Default: "0.0.0.0" Alternative DNS In this field you can give the device the desired alternative DNS IP address in case the primary DNS is not reachable. Example: "195.186.4.111" Default: "0.0.0.0" Syslog Address Destination address for syslog messages sent by the BCL program via the SYSLOG command. Set this to your syslog logging machine, if your syslog messages are recorded centrally. If set to 0.0.0.0, syslog messages are broadcast. Default: "0.0.0.0" DHCP Host Name Name of the device sent in DHCP request. If left empty, a name based on the device's MAC address is generated automatically. Enter up to 15 characters. Web Server Port Defines the port where the webserver of the Barix device can be reached. If set to "0" the default HTTP port (80) is used. "); &LState(2,"%s",28,17,"-->"); Default Ethernet Port On devices with dual-ethernet connection this parameter selects the default port to be used. In most cases selecting ETH1 is suitable, however some devices (e.g. the PS16) provide Power-over-Ethernet (PoE) functionality on ETH2. If you change this parameter do not forget to connect the ethernet cable to the proper port on the rear of the device. Default: "ETH1" SNMP System Name SNMP MIB entry for system name (system.sysName.0) SNMP System Location SNMP MIB entry for system location (system.sysLocation.0) SNMP System Contact SNMP MIB entry for system contact (system.sysContact.0) This parameter can be queried using any SNMP browser but can not be updated.
Help BARP Control BARP Station ID Enter here the BARP system ID of this master station. The ID is used from the clients to identify the source of the control messages in multimaster environment. Default setting is "1001". Paging Priority Enter here the priority of the audio messages sent by this master station. This setting is useful in multimaster environment when a client receives audio messages from many masters simultaneously. In this case the client will play the stream with the highest priority. The priority must be in the range [1-254]. Priority "0" (the highest) is reserved for emergency priority port, priority "255" (the lowest) is reserved for BGM. Default setting is "127". BARP Broadcast Address By default the icclient uses broadcast to listen/send on the BARP ports. Modify the BARP IP address to use multicast if communication across different networks is desired, or if your LAN policy is not allowing broadcast. Default setting is "0.0.0.0". BARP Audio Port Enter the BARP port number to which the master will send audio for paging and established calls. In the multicast port and address are configured, this port will be used only for incoming calls. Paging will be done using the multicast group. Default setting is "5555". BARP Control Port Enter the BARP port number to which the master will send control messages. Default setting is "5556". BARP Status Port Enter the destination port number where the master will listen for BARP status messages. Default setting is "5557".
Help Audio Audio Format Choose between different encoding types and sampling frequencies ("µ-law" or "A-law" at 8 or 24 kHz). Default setting is "µ-law 8 kHz". IMPORTANT: If you change the encoding audio format don't forget to provide correct audio "ring" files! Acoustic Echo Cancellation Choose between "On" and "Off". Default setting is "Off". Note: this options is visible/available only for hardware that supports AEC. Input Source Choose the desired input source. Default setting is "Mic". Duplex Mode Choose the desired mode of operation. Default setting is "Full". Hands Free When set to yes, and HDX mode is enabled, the talk/listen mode can be voice controlled. In Intercom mode, if the voice level exceeds the one set in "Input Trigger Level", the master is switching in talk mode, and the client in listen mode. In Page mode, the Page key needs to be pressed once (instead of press and hold) to activate the paging, and pressed again to stop. Default setting is "No". Hands Free Keys The function of the keys changes depending upon the device and the configuration (Full/Half duplex):
Function | FD Key | HD Key
PS16
Accept Call (IC) | 1 | 1
Reject Call (IC) | 3 | 3
Close Call (IC) | 1 or 3 | 3
Open Relay (IC) | 2 | 2
Start Paging | 2 (blinks whilst Paging)
Stop Paging | 2
PS1 and other 2 button Annuncicoms
Accept Call (IC) | A(1) | A(1)
Close Call (IC) | A(1) | A(1)+B(2)
Open Relay (IC) | B(2) | B(2)
Start Paging | B(2)
Stop Paging | B(2)
Input Trigger Level Triggering input audio level if "Handsfree" mode is selected. Accepted range: 0-32767 Default setting is "1000". Inactivity Timeout Sending of the audio stream in Handsfree mode stops after this number of milliseconds of no input audio signal. Default setting is "1000". Microphone Gain Microphone gain dB, increase if your microphone is too faint, decrease if it's too loud or overdriven. Default: "21 dB". A/D Amplifier Gain A/D converter preamplification in dB. Increase if the audio signal too faint, decrease if it's too loud or overdriven. Default: "0 dB". Default Volume Choose between "0%" and "100%" in 5% steps. Default: "50%".
Help Incoming Call Call Master by Configures the way the master is being called. If set to "ID" then the call is ignored if the destination ID in the call request is not the same as the one of the master. When set to "IP Address", the master reacts on unicast, or broadcasted call requests. The destination ID check is ignored in this case. Default is "BARP ID". Unattended Mode Enables or disables the unattended mode. When enabled, the "Unattended on call after" becomes visible, and can be configured. Disabling the unattended mode is recommended when using the master in a multimaster environment because if any of the masters is in unattended mode, it may always pickup the incoming call thus preventing the other masters to get the call. When disabled, pressing the unattended mode key enters the master in a "Call reject" mode Default is "Enabled". Unattended Timer Configures the number of seconds after the device switches to "unattended mode" during a call. Minimum value allowed is 3, maximum is 60. Default is "20".
Help Paging Group 1 to 8 Address Map Configures the address bitmask containing the clients to be paged for that group. Up to 128 clients may be selected, and the current number of the selected clients for each group is shown. Click on the corresponding "View/Modify" button to open the map configuration page for this group. Default is 10 stations selected for every group "1 to 10 for group 1, 11 to 20 for group 2 and so on.". Audio Multicast Socket Configures the multicast group socket, as IP:PORT, for paging. As IP, it has to be within the range 224.0.0.0 - 239.255.255.255. If set to "0.0.0.0", then the default broadcast address is used. Port is ignored if the IP is set to "0.0.0.0" Default is "0.0.0.0:12345" - use broadcast.
Help I/O Control Relay 1 Control Configures the relay behavior. The relay can be either off ("always off"), on while an incoming call is pending ("relay while ringing") or on while a call is in process ("relay while talking"). Default is "always off". LED Status Configures the device front panel led behavior for the devices that have a led panel. Default is "Input State".
Help SECURITY SETTINGS Reset Function Enable or disable the "Reset" function on the Reset button and on the WEB UI. In order to restart the device press the Reset button once. Default: "enabled" Factory Defaults Enable or disable the "Factory Defaults" feature, applied from both web UI "Defaults" page and device front panel Reset button. In order to revert all settings to factory defaults click on the "Defaults" web UI page, or keep the Reset button pressed until the red LED starts blinking (approx. 10 seconds). Default: "enabled" Update Function Enable or disable the WEB Update function of the device. If the Update function is disabled, the only way to update the firmware is to use the serial rescue. Default: "enabled" Set Password This is visible as long as no password is set. Enter a password (up to 25 characters) and hit the "Apply" button. After the restart you should close the browser window and open a new browser window. You will be asked to supply user name and password. The user name can be omitted but the password has to be supplied in order to see the web configuration. Old Password / New Password These fields are visible as long as a password is set. To allow free access (clearing the password) enter the old password and leave the field "New Password" empty, then hit the "Apply" button. After the restart you will not be asked for user name and password anymore. To change the password enter the old password and enter the new password in the field "New Password", then hit the "Apply" button. After the restart you will be asked for user name and password. The user name can be omitted but the new password has to be supplied in order to see the web configuration.
Read the Intercom Master/Client README for the system description, configuration and instructions to use. To store changed settings click on "Apply" in the left panel. The device will restart with the new setting.