&LSetup(3,"%s",130,D,0," ");

NETWORK SETTINGS
Use SonicIP® | Yes No
IP Address | . . .
Netmask | . . .
Gateway IP Address | . . .
Primary DNS | . . .
Alternative DNS | . . .
Syslog Address | . . .
DHCP Host Name |
Web Server Port | ");&LState(2,"%s",28,17,"-->");
Default Ethernet Port |
SNMP System Name |
SNMP System Location |
SNMP System Contact |

BARP CONTROL
BARP Station ID |
Paging Priority |
BARP Broadcast Address | . . .
BARP Audio Port |
BARP Control Port |
BARP Status Port |

AUDIO
Audio Format |
Acoustic Echo Cancellation | On Off
Input Source | Line Mic
Duplex Mode | Half Full
Hands Free | Yes No
Input Trigger Level |
Inactivity Timeout | msec
Microphone Gain | dB
A/D Amplifier Gain | dB
Default Volume | %

INCOMING CALL
Call Master by | IP Address BARP ID
Unattended Mode | Enabled Disabled
Unattended Timer | secs

PAGING
Group 1 Address Map | &LSetup(1,"%u",858,B); clients selected
Group 2 Address Map | &LSetup(1,"%u",859,B); clients selected
Group 3 Address Map | &LSetup(1,"%u",860,B); clients selected
Group 4 Address Map | &LSetup(1,"%u",861,B); clients selected
Group 5 Address Map | &LSetup(1,"%u",862,B); clients selected
Group 6 Address Map | &LSetup(1,"%u",863,B); clients selected
Group 7 Address Map | &LSetup(1,"%u",864,B); clients selected
Group 8 Address Map | &LSetup(1,"%u",865,B); clients selected
Audio Multicast Socket | . . . :

I/O CONTROL
Relay 1 Control |
LED Status |

SECURITY SETTINGS
Reset Function | Enabled Disabled
Factory Defaults | Enabled Disabled
Update Function | Enabled Disabled
&LSetup(3,"%s",130,D,0," Set Password | "); &LSetup(3,"%s",130,D,!0," | Old Password |
New Password | ");