&L(0,"*",21);
ETHERSOUND

This device can be switched to an alternative firmware image featuring an Ethersound ES-100spkr decoder.

In Ethersound mode all IP functionality is turned off and the device can be controlled only using the ES Control software or any other ES-100 control program.
The device will not be accessible via IP or the WEB UI any more.

Switching back from Ethersound to IP based functionality can only be achieved manually by physically pressing the reset button on the device.

Do you really want to switch to the Ethersound firmware? Click the below link to confirm.

Switch to the Ethersound firmware