&LSetup(3,"%s",1088,B,0,"SIP Phone"); &LSetup(3,"%s",1088,B,1,"SIP Door Station"); &LSetup(3,"%s",1088,B,2,"SIP Paging End Point"); &LSetup(3,"%s",1088,B,3,"SIP Paging Gateway"); &LSetup(3,"%s",1088,B,4,"SIP Monitoring Point");
APPLICATION STATUS
Application Mode | The device is still booting ... | SIP Mode | Peer to Peer
SIP PBX | &LSetup(4,"%s",1020,S);
SIP ID | &LSetup(4,"%s",905,S);
Time till next Registration | &LBAS(1,"%lu",sregt); seconds
Call State | Idle | Calling out | Getting incoming call | In active call | Playing notification message | Playing busy tone | Playing beep tone
Remote Party | &LBAS(1,"%fs",srmt_party$);
P2P Remote Party | &LBAS(1,"%fs",srmt_party$);

AUDIO STATUS
Current Set Volume | &LBAS(1,"%u",svol); %
Left Output Peak Level | &LBAS(1,"%d",spoll); dBFS
Right Output Peak Level | &LBAS(1,"%d",spolr); dBFS
Left Input Peak Level | &LBAS(1,"%d",spill); dBFS
Right Input Peak Level | &LBAS(1,"%d",spilr); dBFS

DEVICE & X8 I/O STATUS

&LState(2,"%s",28,!32,"");