&LSetup(3,"%s",130,D,0," ");

NETWORK SETTINGS
Use SonicIP® | Yes No
IP Address | . . .
Netmask | . . .
Gateway IP Address | . . .
Primary DNS | . . .
Alternative DNS | . . .
Syslog Address | . . .
DHCP Host Name |
Web Server Port | ");&LState(2,"%s",28,17,"-->");
Default Ethernet Port |
SNMP System Name |
SNMP System Location |
SNMP System Contact |

SIP PROTOCOL SETTINGS
Peer to Peer | No Yes
SIP Server (PBX) |
SIP ID (username) |
SIP Password (secret) |
Listen SIP Port |
Listen RTP Port |
Default REGISTER Time |
Send NAT-keepalives | No Yes
Periodically Renew DNS | No Yes
Registration Fail Timeout | seconds
Call Timeout |
Debug Mode | Off On
CIP PROTOCOL SETTINGS
CIP Port Number |
SIP Groups |
SIP Display ID |

OUTBOUND CALL SETTINGS
Call on Level | No Yes
Call on Level ID |
Level Threshold |
Close on Level |
Auto Hangup Time |
Beep on Call Answer | Off On
Call on Device Inputs
Input 0 Call ID |
Input 1 Call ID |

INBOUND CALLS
Input Buffer Level | ms
Phone Pickup Mode |
Pick-up/Hang-up Timeout | seconds
Stream Timeout | minutes
Beep on Call Answer | Off On
DOOR AND RELAY CONTROL
Enable Relay |
Door Open Code |
Open Door Relay for | seconds

AUDIO SETTINGS
Input Source | Line Mic
Encoding |
Volume | %
Microphone Gain | dB
A/D Amplifier Gain | dB
Acoustic Echo Cancellation | Off On
Talk Mode | FDX HDX
Output Trigger Level |
Trigger Level Timeout | ms

CONTROL INTERFACES
Use Serial Port For |
&LSetup(3,"%s",1084,B,2,"Serial GW address:UDP port"); &LSetup(3,"%s",1084,B,3,"Serial GW TCP port"); &LSetup(3,"%s",1084,B,4,"Serial GW address:TCP port"); | . . . : |  |
Serial Port 1 Settings
Baud Rate |
Data Bits |
Parity |
Stop Bits |
Flow Control |

SECURITY SETTINGS
Reset Function | Enabled Disabled
Factory Defaults | Enabled Disabled
Update Function | Enabled Disabled
&LSetup(3,"%s",130,D,0," Set Password | "); &LSetup(3,"%s",130,D,!0," | Old Password |
New Password | ");