Help Profiles page This page lets you easily set the application for a given purpose. When a predefined setting is selected, the nonrelevant settings are set to defaults, so use this feature with caution. After applying the predefined settings, the SIP client can be additionaly customised for the shown properties only. All profiles have in common access to the complete set of settings from the following sections: - SIP Protocol Settings - Door Settings - Control Interfaces Settings In addition, each profile provides extra customisation settings. The following profiles are available: SIP Phone This is the typical use of the SIP client. In this mode you can: Establish a full-duplex phone communication; Call up to 16 (with X8 attached) IDs; Select the audio input; The following additional options are enabled in this mode: - Close on timeout; - Close on Input 0-7 and X8 Input 0-7; - Input audio buffer level; - Input audio source; - Encoding; - Volume; - Mic and AD gains SIP Door Station The device is to be used as a door intercom station. Pushing the button causes the device to ring, and closes the call automatically after some time if not answered. In this mode the SIP client can be used in half duplex mode with AI Phone door panels. The phone pickup mode is preset to "auto answer" and cannot be changed. The following additional options are enabled in this mode: - Close on timeout; - Close on Input 0-7 and X8 Input 0-7; - Input audio buffer level; - Input audio source; - Encoding; - Volume; - Mic and AD gains; - Talk mode (HDX or FDX); - Output trigger level and trigger level timeout for the Voice Activity Detection (VAD); - AI Phone support (On/Off)