Help

These settings adjust the table entries.
Table
There are up to 8 entries in a table. Each entry can be configured to stream to a device, a multi- or broadcast address or to be a listener (server).
The numbered links will allow you to configure additional tables which can be selected over the command interface during operation.
Conn. type
Choose the type of connection:
"not used" for unused entries
"Internet Radio" for an internet radio station (1 user) (default)
"Raw UDP" for a UDP connection
"Raw TCP" for a TCP connection
IP # # # #
Enter 4 values of the entry IP address e.g.:
"0.0.0.0" for unused entries (except when the connection type is set to UDP it will be broadcasted e.g. "192.168.0.255")
"0.0.0.0" for connection TCP + Port if this device is used as a TCP listener waiting for a connection from a streaming device. (default)
"192.168.0.34" for a directed connection
"192.168.0.255" for a broadcast
Default settings:
Entry # 1 in table 1"Raw UDP 0.0.0.0:0". This means it is UDP broadcasting on port 3030!
All other entries are set to "not used" except for table 1 where all entries are set to "Internet Radio 0.0.0.0:0".
Port #
Enter the port number for each entry (between "0" and "65535"). If this port is set to "0" then the default ports are used (Internet Radio "80", TCP "2020", UDP "UDP Receiver Port" or if "0" then "3030").
Default setting is "0".