&L(0,"*",1);

AUDIO Input Source Choose the desired input source. All input sources except "Line stereo" are mono. &LState(1,"%s",6,B,!19," Default setting is "Mic". Audio Format Select encoding (data) format and sampling frequency. The formats are: MPEG, PCM (uncompressed digital audio), uLaw (G.711), A-Law (G.711). Default setting is "MPEG2 / 22.5 kHz". STREAMING Streaming Mode "send always" will stream always "send on TALK" will stream if the TALK button (command) is pressed "send on Level" will stream if the incoming audio signal is above the Trigger level "auto answer" will stream back for the Post Trigger Play duration after a stream has been received "receive only" can receive a stream but will never send one Default setting is "send on TALK". STREAMING DESTINATION Configure the first streaming destination in Table 1 For other Table entries and the option "to origin source" please refer to the advanced settings. Conn. type Choose the type of connection: "not used" for unused entries "Internet Radio" for an internet radio station (1 user) (default) "Raw UDP" for a UDP connection "Raw TCP" for a TCP connection IP # # # # Enter 4 values of the entry IP address e.g.: "0.0.0.0" for unused entries (except when the connection type is set to UDP it will be broadcast, e.g. "192.168.0.255") "0.0.0.0" for connection TCP + Port if this device is used as a TCP listener waiting for a connection from a streaming device. "192.168.0.34" for a direct connection "192.168.0.255" for a broadcast Default settings: "Raw UDP 0.0.0.0:0". This means it is UDP broadcasting on port 3030! Port # Enter the port number (between "0" and "65535"). If this port is set to "0" then the default ports are used (Internet Radio "80", TCP "2020", UDP "UDP Receiver Port" or if "0" then "3030"). Default setting is "0".