Help
Configure the two serial ports.
Serial speed
Select the serial transmission speed in Baud (bits per second).
Default: "9600"
Data bits
Select the number of serial data bits.
Default: "8"
Parity bit
Select the parity bit settings.
If enabled select Even or Odd parity.
Default: "disabled"
Stop bits
Select the number of serial stop bits.
Default: "1"
Flow control (RS-232 only)
Select the RS232 flow control. The options are: "None", "Software" for XON/XOFF flow control or "Hardware" for RTS/CTS flow control.
Default: "None"
Local port
Define the Port on which the serial gateway can be accessed using TCP.
Default: "10001" for RS-232, "10002" for RS-485/422
Enter "0" to disable TCP access and to free TCP handles for BCL application use
Disconnect Tout
Defines the time in seconds after which the TCP connection to the local serial port will be closed due to inactivity.
Enter "0" to disable the Disconnect Timeout (default).
Enter "1" to "255" to enable the Disconnect Timeout.