Help
SNMP
Barix Barionet 50 can issue a specific SNMP trap triggered by a digital input.
Trap Receiver
Enter the 4 values of the desired SNMP Trap receiver IP address e.g.:
"0.0.0.0" for no receiver
"192.168.0.12" for a specific receiver
"192.168.0.255" for a subnet SNMP broadcast
Repeat time
When an input is active the trap will be issued repeatedly with this time in seconds until the input becomes inactive.
Enter "0" to deactivate repetition (results in two traps being sent, one for an input going active and one for it going inactive)
Trap
For each input select if a trap should be issued when the state changes.Default setting is "No".
SNMP definition file (Private MIB)
In order to use the SNMP functions a private MIB definition file called Barionet.MIB is needed.
View MIB in the browser or download zipped MIB file