&L(0,"*");

Versions
Please report this version information when requesting help from support@barix.com
Firmware | V&LSetup(1,"%1V",0);
Web UI | V&LSetup(9,"%02x","BARIO50APPVERSION",1);.&LSetup(9,"%02x","BARIO50APPVERSION",0);
Setup | V&LSetup(1,"%02x",4);.&LSetup(1,"%02x",5);
I/O Drivers | V&LSetup(15,"%02x");.&LSetup(16,"%02x"); 20&LSetup(20,"%02x");&LSetup(21,"%02x");&LSetup(22,"%02x");
Bootloader | V&LSetup(7,"%02x");.&LSetup(8,"%02x");
Update
Please read the help instructions on the right side first. Before you click the link below note that the update process can only be canceled by power cycling the device. Clicking the back button in your browser will produce invalid content. Please click here to continue