APPLICATION SETUP: Digital I/O & Serial Tunnel Version &LBAS(1,"%fs",vers$);

RS-232 TUNNEL
Server settings
Local port |
Disconnect Tout | seconds
Client settings | (disable Server first! See help.)
Remote IP Address | . . .
Remote TCP Port |
Reconnect interval | seconds
I/O TUNNEL
Remote IP Address | . . .
Tunneling UDP Port |
Send Interval | seconds
Remote Input | Local Output Action
Input 1 |
Input 2 |
Input 3 |
Input 4 |
Input 5 |
Input 6 |
Input 7 |
Input 8 |
Communication loss |