&L(0,"*",2);

SETTINGS

NETWORK | SERIAL | I/O | CONTROL | SNMP | TIME | TEMP | SECURITY |

GENERAL
WEB server port |
BCL Program Name |
Lockdown mode |
Modbus/TCP timeout | seconds
COMMAND API
UDP command port |
TCP command port | Timeout seconds
I/O STATE INFO
UDP info send to | . . . (0.0.0.0 for no info)
UDP destination port |
UDP interval | seconds
TCP initial I/O state subscriptions |
TCP add I/O state subscriptions |
SYSLOG
Syslog Server | . . .
Syslog Debug Level | Flags