Help
IP Address
Enter the 4 values of the desired device IP address e.g.:
"0.0.0.0" for automatic discovery (DHCP, IPzator™, AutoIP).
"192.168.0.12" for a static IP address.
Netmask
Enter the 4 values of the desired netmask e. g.:
"0.0.0.0" will use the standard netmask matching the IP address
"255.0.0.0" for a class A network
"255.255.0.0" for a class B network
"255.255.255.0" for a class C network
Gateway IP Address
Enter the 4 values of the desired Gateway IP address e. g.:
"0.0.0.0" for no Gateway
"192.168.0.1" for a specific Gateway in order to access the Internet or a WAN
DNS Server IP Address
Enter the 4 values of the desired Domain Name Server IP address to enable URL domain name to IP address look up e. g.:
"0.0.0.0" for no DNS Server
"192.168.0.1" for a reachable DNS Server
DHCP Host Name
Name of the device sent in DHCP request. If left empty, a name based on the device's MAC address is generated automatically (a "C" followed by the last 6 digits of the MAC address, e.g. "C8041B8"). Enter up to 15 Characters.