Help
NTP Server IP Address
Enter the 4 values of the desired NTP Server IP address e. g.:
"0.0.0.0" for no NTP Server
"192.168.0.1" for a NTP Server in a LAN
When a valid NTP Server is given, the Barionet will set the internal clock accordingly at start up and will synchronize again approximately every 10 hours.
Onewire RTC
If a Real-Time-Clock chip like the DS1904L is connected to the 1-wire bus then the bus address is shown. The internal clock will take the time from this RTC on start up..
Time Zone
Enter the time zone information for your geographic location in order to display the correct local time.