0418
/* * * * * * * * * * * * * * * * * * * * * * * * * * *
Vers  Date     Who  What
<==== Log Truncated to save space ===>
04.10 12.10.10 PK - realtime status using JS
                  - #052.80 VU meter on the UI
                  - #052.65 error 400 when changing volume during priority msg
      16.10.10 PK - #052.75 configurable behaviour on USB backup switchover
      18.10.10 PK - #052.05 UDP and TCP command ports plus respective parameters in update.ini
      01.11.10 PK - new parameter "usb_backup_switch_immediately" in update.ini
                  - #052.88: balance settings
04.11 09.11.10 PK - #053.14: volume control in 1% steps
                  - Setup version incremented to 1.3
                  - #035.06: network settings checked by javascript
      14.11.10 PK - fixed wrong netmask chec
      31.01.11 PK - #52.92: homepage not updating in MS IE7 - using "lightgrey" instead of "lightgray"
      18.02.11 PK - #52.93: removed password protection from rebooting.html; causing 401 after setting password in Configuration
      21.04.11 PK - #52.98: Exstreamer 105 detection
      12.05.11 PK - #100.02: Exstreamer 205 detection
      17.05.11 PK - #051.02: boot target 2K for multi package
      19.05.11 PK - #052.82: triggered playlist in priority settings; new parameter S570
                  - #100.01: discover.txt for IC Graph discovery c=65535 command
      20.05.11 PK - default channel number 1
                  - Playback Settings renamed to Audio & Playback Settings
                  - #100.03: line-in gain settings on Exstreamer 205
      23.05.11 PK - #100.05: volume offset
      24.05.11 PK - #052.94: uptime in dd hh mm ss, current song title and media format in the Status page
04.12 06.09.11 PK - #100.11: runtime volume control on priority port
      22.11.11 PK - #100.24: endless countdown on update page if FW update disabled
                  - firmware upload help simplified and cleaned up
04.13 17.01.12 PK - #100.26: added file "inputs.txt" containing I/O state of 8 digital inputs
      18.01.12 PK - #100.29: relay control on priority port: new option "priority" in relay control, current "audio" option renamed to "stream" and is triggered only on non-priority stream
      26.01.12 PK - #100.30: extended information in ASCII discovery (discover.txt)
04.14 29.02.12 PK - #100.34: IPAM type added to Status page
      13.03.12 PK - HW and IPAM type displayed in text using auto-generated javascript functions
      21.09.12 PK - #100.18: configurable audio buffer size
                    #100.44: remote update availability and flash memory size added to status page
04.15 17.01.13 PK - #100.48: new Barix logo
      01.02.13 PK - #100.48: added favicon.ico with the new logo
      08.03.13 PK - #100.49: configurable SNMP read community using password nr.4
                  - #100.50: configurable SNMP SysName and SysLocation
      19.03.13 PK - SNMP community, sysName and sysLocation added to status page
04.16 13.11.13 PK - #100.38: configurable fade-in period
      19.11.13 PK - new Setup parameter W376 for Remote Content Update
      12.12.13 PK - configurable content update folder
      13.12.13 PK - updater module added into version list
      21.11.14 PK - #100.70: added codec type to the Status page
      24.11.14 PK - #100.69: configurable syslog address for remote update
      06.01.16 PK - #100.59: help text correction of "Relay Output" controlled by "Stream"
      07.01.16 PK - #100.73: SNMP RO community added into update.ini
      08.01.16 PK - #100.27: relay control via the R= command
                  - corrected wrong relay control values for relays 7 and 8
04.17 28.07.19 PK - use | as a field separator instead of a semicolon in realtime_status.txt to avoid collision with HTML escaped chars
04.18 24.08.21 ASI- Updated the remote.ini file to support the new IR remote control
*/
