Help Status page Overview of the status of the unit. Player Status - IDLE: No audio stream is received. - BUFFERING: Audio stream is requested from the source, internal buffer is filled. - PLAYING: Audio stream is received from the source and played back. - PRIORITY: Audio stream on the priority port is received and played back. - STAND-BY: Unit is in stand-by mode, network activity is reduced to minimum, no audio stream is received. Source Current streaming source: URL1, URL2 or URL3. Channel Currently selected channel number. Shuffle Play a playlist in a random order.
= Off | = On
Repeat Repeat the current song in the playlist.
= Off | = On
Stream URL address of the actual stream. -PRIORITY: Priority message is received. Title Title of the currently played song/Name of the internet radio station. Audio Output Bitrate Data rate of the stream in kilobits per second. Buffer The number [in bytes] and the graphical meter show the utilisation of the internal buffer. Max. value is 65532 bytes. Volume Current output volume in per-cent. Peak Left and Right The numbers [in dB full-scale] and the graphical VU meters show the peak values of the audio outputs. Max. value is 0 dB. Control outputs
= Idle | = Active
= Not available on the hardware