Help
Updating files
Download the desired firmware package (ZIP file) from www.barix.com and unpack the archive to a local drive. Click "Browse..." and locate the compound.bin within the firmware package.
Click the "Upload" button and wait for a confirmation of the upload.
Do not interrupt the upload process, reset or power off the device until the firmware is loaded.
After the file completely loads, click on update and then press the "reboot" button to restart the device with the new firmware.
The device takes a few seconds to reboot.