Help BASIC SETTINGS SIP PROTOCOL Peer to Peer Choose whether peer to peer calls should be allowed. NOTE:When using P2P, the device uses always the default SIP (port 5060) and RTP (port 5004) ports. Make sure the remote peers are configured to listen on the default ports as well. SIP Server (PBX) Enter here the hostname/IP address of the SIP server. SIP ID Enter the SIP ID (username) that has been created for this device. SIP Password Leave this field empty if the PBX doesn't require authentication. OUTBOUND CALLS Call on Level If enabled, call can be initiated by audio level. If set to "Yes", then Call on Level ID, Level Threshold and Close Call on Level options are also visible. NOTE: Call on level is unsupported with "Background Music" enabled. Call on Level ID SIP extension of the device that will be called on audio level detection. In case of using "Peer to Peer" mode, enter here the ID and the IP address of the remote peer, for example: 1234@192.168.0.123 Level Threshold Minimal audio level to initiate a call. If the input audio level reaches at least the configured threshold, a call will be initiated. The same threshold level is used to terminate the call if the Close Call on Level option is enabled Values: 0 to 32767. Default: 1000 Close Call on Level When enabled, and the input peak level is below the level threshold for the configured amount of time, the call is terminated. Values: 5 to 30 seconds. Default: 0 (disabled) Call on Device Input 0 Extension to be called when input 0 is closed. In case of using "Peer to Peer" mode, enter here the ID and the IP address of the remote peer, for example: 1234@192.168.0.123 INBOUND CALLS Phone Pickup Mode Choose how calls should be answered. autoanswer: the call is auto-answered. autopick up after timeout: in this mode the bell button is used to answer and terminate a call. If the call is not answered inside "Pick/hang up after" time period, the device will answer. autohang up after timeout : (default) in this mode the bell button is used to answer and terminate the call. If the call is not answered inside "Pick/hang up after" time period, the device will decline the call. not callable: in this mode incoming calls will be declined. Pick/Hang-up Time Set pick/hang up delay if no answer. Only active if the phone pickup mode is set to manual.