Help Home page Gives an overview of the most important settings of the unit. APPLICATION STATUS Application Mode Shows the current mode of the application, and may take the following values: - Device is still booting ... The Boot process has not finished yet. - SIP mode The device is in SIP mode. The SIP server name, and the SIP ID are also shown in this case - Peer to peer mode The device is in P2P mode, and configured to call to only one remote peer. Incoming calls will be accepted only from this peer. Time till next Registration Shows the remaining time till the next registration attempt. The current registration status is shown with different colours of the text:
| Device not registered
| Registration in progress
| Device registered
Call Status Shows the current call state, and may take one of the following values: - idle: No audio stream is received, and the SIP client is accepting calls - Getting incoming call: The SIP client has received an INVITE message and is ringing. The ID of the remote party is also displayed - Outgoing call: The SIP client has initiated an outgoing call, and the remote party ID is displayed as well. - In active call: The SIP client is in a call session with the displayed remote party DEVICE AND X8 I/O STATUS Displays the available I/Os of the device, and of X8 (if attached). A message "X8 not connected" appears when X8 is not detected. Device I/O Device I/O enumeration, bit "0" correspond to the first device input, for example IN0 for Annuncicom 100. Inputs &LState(2,"%s",28,32,""); &LState(2,"%s",28,!32,""); Relays
Monitors the device relays, indicated with the following states:
| = Relay activated |  | = Relay not active
= Not available on the hardware
NOTE: please read the ABCL Firmware documentation and the product manual to understand how input, output and relays are mapped, and where they are available. X8 I/O Status X8 I/O enumeration, bit 0 corresponds to pin 9 of J1 connector. Please refer to X8 manual for additional information. X8 pin configuration
The pin configuration is indicated with the following icons:
| = Set as input |  | = Set as output
For more information how to change the pin configuration please refer to X8 manual. X8 Input Register X8 input register status. Please refer to X8 manual for additional information. X8 Output Register X8 output register status. Please refer to X8 manual for additional information. AUDIO STATUS Shows the status of the following audio parameters: - Volume: Displays the current volume in % - Left Output Peak Level Displays the current left ouput peak level in dBFS (dB full scale) - Right Output Peak Level Displays the current right output peak level in dBFS (dB full scale) - Left Input Peak Level Displays the current left input peak level in dBFS (dB full scale) - Right Input Peak Level Displays the current right input peak level in dBFS (dB full scale)