&L(0,"*",5);

Active Profile | &LSetup(3,"%s",1088,B,0,"SIP Phone"); &LSetup(3,"%s",1088,B,1,"SIP Door Station"); &LSetup(3,"%s",1088,B,2,"SIP Paging End Point"); &LSetup(3,"%s",1088,B,3,"SIP Paging Gateway"); &LSetup(3,"%s",1088,B,4,"SIP Monitoring Point");
Call State |
Remote Party | &LBAS(1,"%fs",srmt_party$);
Registration Status |
Current Set Volume | &LBAS(1,"%u",svol); %
Left Output Peak Level | &LBAS(1,"%d",spoll); dBFS
Right Output Peak Level | &LBAS(1,"%d",spolr); dBFS
Left Input Peak Level | &LBAS(1,"%d",spill); dBFS
Right Input Peak Level | &LBAS(1,"%d",spilr); dBFS