&LSetup(3,"%s",130,D,0," "); &LSetup(3,"%s",122,D,0,"

NETWORK SETTINGS
Use SonicIP® | Yes No
IP Address | . . .
Netmask | . . .
Gateway IP Address | . . .
Primary DNS | . . .
Alternative DNS | . . .
DHCP Host Name |
Web Server Port |
Type of Service/DSCP |

AUDIO SETTINGS
Input Source |
Audio Format |
MPEG Bitrate Mode |
MPEG Bitrate |
MPEG Encoding quality |
ADVANCED ENCODER SETTINGS &LState(1,"%s",6,B,35," &LState(1,"%s",6,B,32," &LState(1,"%s",35,B,2,"
MP3 Bit Reservoir | &LState(1,"%s",35,B,2,"

STREAMING SETTINGS
Streaming Mode |
Trigger Level | - dB
Pre Trigger Start | msec
Post Trigger Play | msec
Contact Closure |
Input Polarity | &LState(1,"%s",10,B,<1,"
Buffer Underrun Mode (TCP) |
Stream Packet Strategy |
UDP Tx Source Port |
SHOUTCAST/ICECAST SETTINGS
Own Name |
Radio Path |
Icecast 2 User Name |
icy-url / SIP user |
icy-genre |
Shoutcast stream |
STREAMING DESTINATIONS
# |  | Conn. type | Enter IP Address or Domain Name | Port
1 |  |  |  |
2 |  |  |  |
3 |  |  |  |
4 |  |  |  |
# |  | Conn. type | IP # | # | # | # | Port
5 |  |  | . | . | . | : |
6 |  |  | . | . | . | : |
7 |  |  | . | . | . | : |
8 |  |  | . | . | . | : |

IO SETTINGS
CTS close command |
CTS open command |
SERIAL SETTINGS
Baud rate |
Data bits |
Parity |
Stop bits |
Flow control |
SERIAL GATEWAY
Local port |
Destination IP | . . .
Destination port |

CONTROL SETTINGS
UDP command port |
TCP command port |
TCP connection address | . . .
SNMP SETTINGS
Trap Target IP Address | . . .
Low Audio Level | Left - | Right -
High Audio Level | Left - | Right -
Trap Repeat | Left sec | Right sec
Silence Timeout | Left sec | Right sec

SECURITY SETTINGS
Level | Password | Status
Save Configuration |  | &LSetup(3,"%s",122,D,0,"not ");set
View Configuration |  | &LSetup(3,"%s",130,D,0,"not ");set
Control/Command |  | &LSetup(3,"%s",138,D,0,"not ");set
User Password |  | &LSetup(3,"%s",146,D,0,"not ");set
Icecast/Shoutcast |  | &LSetup(3,"%s",205,B,0,"not ");set
Factory Defaults at Reset |
Listening |
SNMP Community RWrite |
SNMP Community Read |