Help

Read the Digital Message Streamer README for the system description, configuration and instructions to use.
To store changed settings click on "Apply" at the bottom of the page. The device will restart with the new setting.
Volume
Click on the volume bar to change the volume.
Default setting is "60 %".
FTP Server Name
Insert the FTP server name here (max 49 characters).
By default the name is empty.
Resolved FTP Server Address
If the DNS resolution of the FTP server has been successfully completed at boot, you must here its IP address.
FTP User Name
Insert here the FTP login name (max 25 characters).
Default setting is empty (no name).
FTP Password
Insert here the FTP login password (max 25 characters).
Default setting is empty (no password).
FTP Directory
Insert here the FTP directory where your message files and playlist reside (max 25 characters). Enter the path without the starting and the ending slash, like:
my_own/ftp_directory
Default setting is empty (your home directory on the FTP server).
FTP Download Time
Enter here the exact time whe you would like to start downloading the new playlists from the FTP server. Up to three download timers may be defined.
Default setting is 00.00h
NTP Server Name
Insert the NTP server name here (max 49 characters).
By default the name is empty.
Resolved NTP Server Address
If the DNS resolution of the NTP server has been successfully completed at boot, you must here its IP address.
NTP Update Period
Set here how often you would like to have NTP time updated. the NTP server name here (max 49 characters).
Default setting is Every 1 hour
Local Timezone
Select here from the dropdown menu the zone in which you are in. A list of countries belonging to that zone is shown as a tooltip when a certain entry is preselected.
Daytime Saving
Selecting "Yes" adds one hour to your current time zone setting. Please have in mind that there is no automatic daylight saving correction, so you will need to change this setting when needed.
Local Time
The local time as calculated from the device is shown here. Check if it corresponds to the time according to your timezone.
RTP Send Address
Set here the address where you would like to have the messages being sent to. Any unicast or multicast address will work. For broadcast use address "0.0.0.0"
Default setting is 0.0.0.0
RTP Send Port
Set here the port where you would like to have the messages being sent to.
Default setting is 0