Help Network Settings This section allows the configuration of the following device settings: IP address Netmask Gateway DNS Syslog message destination server: if unset (default, set to 0.0.0.0) syslog messages are broadcasted DHCP hostname WEB server listening port Configuration Server 1,2,3 At boot time the application will try to contact the first available configuration server. The first of them that will answer with a valid reply will be used for configuration and reflector services. To see the state of the connection a status string is reported in the "device status" section of the home page. Common cases of unreachable server are: a) No correct gateway has been set. b) No correct DNS server has been set. c) Device is not registered in the server database, that mean that no device realted projects has still been created on the server side. Security Settings This section allows to configure the device password and other security settings. Reset Function Enable or disable the "Reset" function on the Reset button and on the WEB UI. In order to restart the device press the Reset button once. Default: "enabled" Factory Defaults Enable or disable the "Factory Defaults" function on the Reset button. In order to revert all settings to factory defaults keep the Reset button pressed until the red LED starts blinking (approx. 10 seconds). Default: "enabled" Update Function Enable or disable the WEB Update function of the device. If the Update function is disabled, the only way to update the firmware is to use the serial rescue. Default: "enabled" Set Password This is visible as long as no password is set. Enter a password (up to 25 characters) and hit the "Apply" button. After the restart you should close the browser window and open a new browser window. You will be asked to supply user name and password. The user name can be omitted but the password has to be supplied in order to see the web configuration. Old Password / New Password These fields are visible as long as a password is set. To allow free access (clearing the password) enter the old password and leave the field "New Password" empty. Enter the old password in the password field above the "Apply" button as well and then hit the "Apply" button. After the restart you will not be asked for user name and password anymore. To change the password enter the old password and enter the new password in the field "New Password". Enter the old password in the password field above the "Apply" button as well and then hit the "Apply" button. After the restart you will be asked for user name and password. The user name can be omitted but the new password has to be supplied in order to see the web configuration.