&L(0,"*",1);

This page shows the current status of the device.
Several links allow control and allow simulation of button inputs, relay output and control signals of the serial port.
The manual and the technical documentation are available at www.barix.com.
Stream
Shows the streaming mode and the audio format.
Audio
Shows the current Audio Input and Output Peak levels in dB, current volume in % and the audio input source.
Status
Shows the current audio status
Possible states: "IDLE" "INACTIVE", "TALKING", "TALKING SUPPRESSED", "FORCED TALKING", "LISTENING".
Click the "FORCE" link to force the talking (not visible if "send always" mode is configured). This overrides the "TALKING SUPPRESSED" mode, e.g. when another device is talking to this device.
Click the "TALK" link to start talking (not visible if "send always" mode is configured).
Click the "STOP" link to stop talking (not visible if "send always" mode is configured).

The Status indicator has the following meaning:
  - not talking
  - talking
  - forced talking

TABLE
Select the streaming table by its number.
ENTRY
Select "All" for talking to all configured entries within the table. Select a particular number to talk only to that entry.
BUTTON 0 and 1
Shows the status of and controls the button inputs.
Click "SET" to simulate button beeing pushed, click "CLR" to simulate the button beeing released.

The indicator next to "BUTTON" shows the status of the physical input (simulation is not shown!):
  - button released (input not activated)
  - button pushed (input is activated)
  - shortcut on the input (available only on devices supporting supervision)
  - no connection (available only on devices supporting supervision)

&LState(1,"%s",6,B,32," &LState(1,"%s",6,B,!32," &LState(1,"%s",6,B,42," &LState(1,"%s",6,B,!32," Tips
- To configure the device click on the "CONFIGURATION" button.
- The volume slider in the audio section can be used to temporarily change the volume.
- This page can be customized to meet installation requirements. Download the development kit from www.barix.com.