Help
Dallas 1-wire® Temperature sensors
Temperature sensors can be attached to Barionet's 1-wire bus. This page shows addresses (unique IDs) of the detected temperature sensors (in the order of discovery).
Up to 50 sensors can be attached, but only the first 8 are displayed. The complete list of addresses can be retrieved from IO registers 651 to 700.
1-wire devices are detected at the boot-up time of the Barionet.